**Cyclic Triaxial Set up equipment**

|  |  |
| --- | --- |
|  | **Name of the equipment:** Cyclic Triaxial Set up**Make & Model:**HEICO; Model: HS28.630**I-Stem Registration ID-** **……………………..** **Category of Instrument**Geotechnical Engineering**Types of Analysis / Testing**Soil Sample**Application:** Assessing the cyclic strength and liquefaction resistance of soils.**Description of Instrument**Cyclic axial loading with frequency up to 10 Hz. |

**Booking Details**

|  |  |
| --- | --- |
| **Book through I-STEM:** <https://www.istem.gov.in/>**Slot Booking Link**[I-STEM Slot Booking link for External User](https://www.istem.gov.in/) | **Booking available for**Internal and External Both**Requisition form for** [Internals](https://randc.nitc.ac.in/pdf/instruments/civil/CED-REQUISITION_FORM_Internal.pdf)[Externals](https://randc.nitc.ac.in/pdf/instruments/civil/CED-REQUISITION_FORM_Internal.pdf) |

**Contact Details**

|  |  |  |
| --- | --- | --- |
| **Faculty In-charge:** Dr. Kodi Rangaswamy, **Email ID:**ranga@nitc.ac.in, **Phone number:** +91-9846162955 | **Technical Staff:** Nayana P nayanap@nitc.ac.in Lini Ignatius C liniignatiusc@nitc.ac.in Ajith Augusthy ajithaugusthy@nitc.ac.in | **Department**CED**Office Email ID**cedoffice@nitc.ac.in**Location**Geotechnical Lab, Department of Civil Engineering**Lab Phone No**0495-2286245 |

**Features, Working Principle and Specifications**

|  |  |
| --- | --- |
| **Features of the equipment*** Used for conducting Unconsolidated Undrained (UU), Consolidated Undrained (CU), and Consolidated Drained (CD) triaxial tests on soil specimens under dynamic condition
* Allows testing under different confining pressures (σ3) and dynamic loading conditions.
 | **Unique features/Measurement capabilities, if any*** Resilience Modulus can be determined
 |
| **Instrument Technical Description and Major Specifications (This Specifications Limited to Major 5)*** LVDT displacement 0.01mm-50mm
* Load cell 5kN
* Pressure Sensor 0.01kg/cm2 to 10kg/cm2
* Universal Load Cell
* Maximum dynamic load 5kN.
* Frequency – 1 to 10 Hz.
 | **Measurement/Sample specifications:** * 38mm, 50mm and 100mm dia
* All kind of soil samples
 |

**Type of Sample Required for Analysis / Testing (Quantity, Pre-Preparation, State etc.) Guidelines for Sample Submission – User Instructions**

|  |
| --- |
| * All soil sample (Clay, Silt, Sand, etc) minimum 1 Kg
 |

**User Charges Rs. (GST Extra)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Internal** | **External Academic Institutes** | **National R&D Lab** | **Industry** |
| 2000/- per sample | 9000/- per sample | 9000/- per sample | 15000/- per sample |